**ADC**

Prints ADC readings

**Load 090**

Sets load pwm to 90% duty cycle. Supports 0-100. Must be 3 digits, may start with 0.

**Wind 090**

Sets wind pwm to 90% duty cycle. Supports 0-100. Must be 3 digits, may start with 0.

**PV 090**

Sets pv to 090 spi call. Supports 0-128. Must be 3 digits, may start with 0.