**ADC**

Prints ADC readings

**Load 90**

Sets load pwm to 90% duty cycle. Supports 0-99. Does not support 100.